1. Raspberry Pi Connected to the internal network
2. python3 start.py
   1. Checking for connection
   2. Checking for local ip address
   3. IP Scanner for 255.255.X.X
   4. Port Scanner for 502/44818 ports
      1. If exist → send command to HMI (Need to provide the command)